
DMI Wizard 2.0		[ Released version, Date: 06/06/96 ]
------------------------------------------------------------------------------

	Prepare for installation:
	------------------------
	
	1.	To make a Installation Diskette copy INSTALL.EXE, INSTALL.INF
		and DMIWIZ.000 to a floppy. Label the floppy as DMIWIZ.
		
	2.	To install from a hard disk, copy INSTALL.EXE, INSTALL.INF and
		DMIWIZ.000 to the same directory.
		
------------------------------------------------------------------------------

	To Install DMI Wizard 2.0
	-------------------------

	1.	Run INSTALL.EXE
	
	2.	To execute DMIWIZARD 2.0, type DMIWIZ [USER/OEM]
			
			DMIWIZ USER(default)  -  for end user level
				or
			DMIWIZ OEM  -  for oem level
				or simply
			DMIWIZ  -  for end user level
		
------------------------------------------------------------------------------

	Few Tips:
	--------
	
	** DMI Wizard 2.0 needs 384KB memory available in the system after
	   it is loaded. This is due to read 128KB ROM, compressing,
	   uncompressing etc. If the system does not have 384KB memory, DMI
	   Wizard cannot be run. To make it work, do the following.
	   
	   a)	Take out all TSRs from CONFIG.SYS and AUTOEXEC.BAT
	   b)	In CONFIG.SYS, write the following.
	   		DOS = HIGH
			DEVICE = C:\DOS\HIMEM.SYS
			

	** DMI Wizard has Graphical User Interface. To enhance the interface
	   load the DOS Mouse driver before running the utility. But mouse
	   is not a mandatory input device for this utility.
	   
	** If any problem occurs, run DMIDUMP.EXE for further investigation.
	   Also run DMIDUMP.EXE to examine your BIOS DMI implementation. Type
	   DMIDUMP /? for more information.
	   

