Installation of the ES1938/ES1946 AudioDrive for Windows 98

 1. Turn the PC ON.
 2. Insert the Windows 98 CD in a CD-ROM drive (at the certain 
    installation points some Windows 98 CD files that support the 
    devices on the sound card have to be copied).
 3. Wait for Windows 98 boot up.
 4. Windows 98 automatically detects the PCI Multimedia Audio Device 
    and brings up the Add New Hardware Wizard.
 5. The Add New Hardware Wizard will show the ESS Solo-1 PCI Audio 
    Device.  Click next to continue.
 6. At the next screen, check the "Search for the best driver for 
    your device (Recommended)" box, and click next.
 7. At the next screen, make sure that the Floppy disk drives box is
    checked.  Insert the driver disk into floppy drive and click next.
 8. The Add New Hardware Wizard should then display ESS Solo-1 PCI 
    Audio Device (WDM), and the location of the driver should be your 
    floppy drive.
 9. Click Finish, and the Add New Hardware Wizard will then install 
    drivers for the ESS Solo-1 PCI AudioDrive (WDM), ESS Solo-1 
    SoundBlaster Compatible (WDM), and Gameport Joystick by copying 
    files from the floppy diskette and the Windows 98 CD.
10. Installation is now complete.


