
                   =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
                   Adaptec 7800 Family Manager Set v3.02 for Windows 95
                   =-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=


=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=
Welcome to Adaptec 7800 Family Manager Set v3.02
=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=-=

The following information is available in this README file:

   o Supported Hardware
   o Changes From Prior Release
   o Installation Instructions
         Installing the Driver When Installing Windows 95
         Updating the Driver for Windows 95 (Retail Edition)
         Updating the Driver for Windows 95 (OSR2.x)
   o Known Issues
   o Diskette Contents
   o Contacting Adaptec



=-=-=-=-=-=-=-=-=-=
Supported Hardware
=-=-=-=-=-=-=-=-=-=

The following Adaptec SCSI Host Adapters are supported by the 7800 FMS v3.02.  
The first list (Fast/Ultra Adapters) is supported by the AIC78xx.MPD driver, 
while the second list (Ultra2 Adapters) is supported by the AIC78U2.MPD 
driver.

   Fast/Ultra Adapters  Description
   -------------------  -----------
   AVA-2902I            PCI-to-Fast SCSI (non-bootable, internal)
   AVA-2902E            PCI-to-Fast SCSI (non-bootable, external)
   AVA-2903             PCI-to-Fast SCSI (non-bootable, internal, external)
   AVA-2904             PCI-to-Fast SCSI (non-bootable)
   AVA-2906             PCI-to-Fast SCSI (non-bootable, internal, external)
   AHA-2910C            PCI-to-Fast SCSI (non-bootable)
   AHA-2915C            PCI-to-Fast SCSI (non-bootable)
   AHA-2920C            PCI-to-Fast SCSI
   AHA-2930C            PCI-to-Ultra Single-ended SCSI
   AHA-2940             PCI-to-Fast SCSI
   AHA-2940W            PCI-to-Fast and Wide Single-ended SCSI
   AHA-2940AU           PCI-to-Ultra Single-ended SCSI
   AHA-2940U            PCI-to-Ultra Single-ended SCSI
   AHA-2940U Dual       DualChannel PCI-to-Ultra Wide Internal Single-ended SCSI
                        with 50-pin external connector
   AHA-2940UW           PCI-to-Ultra Wide Single-ended SCSI
   AHA-2940UW Dual      DualChannel PCI-to-Ultra Wide Single-ended SCSI
                        with 68-pin external connector

   AHA-2944W            PCI-to-Fast and Wide Differential SCSI
   AHA-2944UW           PCI-to-Ultra Wide Differential SCSI
 
   AHA-3940             MultiChannel PCI-to-Fast SCSI
   AHA-3940W            MultiChannel PCI-to-Fast and Wide SCSI
   AHA-3940U            MultiChannel PCI-to-Ultra SCSI
   AHA-3940UW           MultiChannel PCI-to-Ultra Wide SCSI
   AHA-3940UWD          MultiChannel PCI-to-Ultra Wide SCSI with dual
                        external connectors
   AHA-3944UWD          MultiChannel PCI-to-Ultra Wide Differential SCSI
                        with dual external connectors
   AHA-3940AU           MultiChannel PCI-to-Ultra SCSI
   AHA-3940AUW          MultiChannel PCI-to-Ultra Wide SCSI
   AHA-3940AUWD         MultiChannel PCI-to-Ultra Wide SCSI with dual
                        external connectors
   AHA-3944AUWD         MultiChannel PCI-to-Ultra Wide Differential SCSI
                        with dual external connectors

   AHA-4944W            Quad Channel PCI-to-Fast and Wide Differential SCSI
   AHA-4944UW           Quad Channel PCI-to-Ultra Wide Differential SCSI

   APA-1480             CardBus-to-Ultra Single-ended SCSI

   AIC-7850             Single-chip PCI-to-Fast SCSI
   AIC-7855             Single-chip PCI-to-Fast SCSI
   AIC-7856             Single-chip PCI-to-Fast SCSI
   AIC-7860             Single-chip PCI-to-Ultra SCSI
   AIC-7870             Single-chip PCI-to-Fast and Wide SCSI
   AIC-7880             Single-chip PCI-to-Ultra Wide SCSI
   AIC-7895             Single-chip PCI-to-MultiChannel Ultra Wide SCSI

   Ultra2 Adapters      Description
   ---------------      -----------
   AHA-2940U2 OEM       PCI-to-Ultra2 Wide LVD/Single-ended SCSI 
   AHA-2940U2B          PCI-to-Ultra2 Wide LVD SCSI
   AHA-2940U2W          PCI-to-Ultra2 Wide LVD/Single-ended SCSI
   AHA-2950U2B          64-bit PCI-to-Ultra2 Wide LVD SCSI
   AHA-3950U2B          64-bit PCI-to-MultiChannel Ultra2 Wide LVD SCSI

   AIC-7890             Single-chip PCI-to-Ultra2 SCSI
   AIC-7891             Single-chip 64-bit PCI-to-Ultra2 SCSI
   AIC-7896             Single-chip PCI-to-MultiChannel Ultra2 SCSI
   AIC-7897             Single-chip 64-bit PCI-to-MultiChannel Ultra2 SCSI


=-=-=-=-=-=-=-=-=-=-=-=-=-=
Changes From Prior Release
=-=-=-=-=-=-=-=-=-=-=-=-=-=

Adaptec 7800 Family Manager Set v3.02 features enhancements from
the previous v3.01 version. These features include:

   o Support for a wider variety of Ultra2SCSI PCI ICs and host adapters
   o Support for Windows 98 (See seperate readme)


=-=-=-=-=-=-=-=-=-=-=-=-=-=
Installation Instructions
=-=-=-=-=-=-=-=-=-=-=-=-=-=

If you are performing a first time Windows 95 installation, see the 
"Installing the Driver When Installing Windows 95" section, below.  If 
Windows 95 is already installed on your system, see the "Updating the 
Driver for Windows 95" section.

NOTE: Windows 95 shipped in two different version - the Retail Edition
and the OEM Service Release 2 (or OSR2) Edition.  To determine which 
version you have, follow these steps:

    1 Select Control Panel under Settings from the Start Menu.

    2 Double-click the "System" icon.

    3 Under the "General" tab, it will display the version number of 
      Windows 95 under the System category.
      
    4 If it displays "4.00.950", you have the Retail Edition installed.
      If it displays "4.00.950 B", you have OSR2 installed. 

Both versions function the same, but the process of installing drivers
is different.  Please make a note of this when updating your driver.


Installing the Driver When Installing Windows 95
------------------------------------------------

A fresh Windows 95 installation will attempt to detect all Adaptec 
SCSI host adapters in your system.  If it is unable to do so, follow
the instructions in the "Updating the Driver for Windows 95" section 
below.

(NOTE:  When Windows 95 starts, if "New Hardware Found" is displayed, 
select "Driver from disk provided by hardware manufacturer".  Insert 
your Adaptec 7800 Family Manager Set v3.02 Diskette and type a:\win9x 
as the path; follow the on-screen instructions.)


Updating the Driver for Windows 95 (Retail Edition)
---------------------------------------------------

To update or install the aic78xx.mpd or aic78u2.mpd driver if Windows 95 
is already installed, follow these instructions:


    1 Start Windows 95.

    2 Click the Start button on the Windows 95 task bar, and then
      point to Settings.

    3 Click Control Panel.
    
    4 Double-click the System icon.
    
    5 On the Device Manager tab, click the plus sign next to the SCSI
      controller icon.
    
    (NOTE:  If Windows 95 cannot determine the type of host adapter
    installed in your computer, a yellow question mark labeled Other
    devices appears instead of the SCSI controller icon.  To continue, 
    click the plus sign next to the question mark; a yellow question
    mark labeled PCI SCSI Bus Controller then appears.)
    
    6 Double-click the 7800 Family host adapter you wish to update,
      or if a yellow question mark labeled PCI SCSI Bus Controller
      is displayed, double-click the question mark.
    
    7 Insert the Adaptec 7800 Family Manager Set v3.02 Diskette into 
      drive A:.
      
    8 Select the Driver tab.
    
    (NOTE:  If the version of Windows 95 you are using now displays a 
    window with a Update Driver button instead of a Change Driver button, 
    the remainder of your install procedure is covered in Updating the 
    Driver for Windows 95, Version OSR 2, described below.)
    
    9 Click Change Driver.  You may be asked to select the hardware type;
      if so, select SCSI Controllers.
     
   10 Click the Have Disk button and enter a:\win9x as the path.
      
   11 Click OK.
    
   12 Select the Adaptec 7800 Family host adapter, and click OK.
   
   13 Again, click OK.  The driver is now installed.
   
   14 You must restart your computer for the changes to take effect.  Click 
      Yes to restart your computer.  Click No to return to the system 
      properties window.


Updating the Driver for Windows 95 (OSR2.x)
-------------------------------------------

This section covers the remaining steps to updating the driver on
Windows 95 OSR2.

(NOTE:  If you have not already done so, follow the instructions in
"Updating the Driver for Windows 95" section above.)

    1 Click Update Driver.
    
    2 Insert the Adaptec 7800 Family Manager Set v3.02 diskette into driver 
      A:.
    
    3 In the Update Device Driver Wizard, select Yes, and click Next.
    
    4 Select Other locations.
    
    5 Under the Location edit box, type a:\win9x, then click OK.
    
    6 Click the Finish button.
    
    7 At the message "Please insert the disk labeled '7800 Family Manager 
      Set v3.02 Installation Disk'."  Insert the Adaptec 7800 Family 
      Manager Set v3.02 diskette and click OK.
    
    8 Another dialog box, Copying Files, appears with the message "The file
      'AIC78XX.MPD' or 'AIC78U2.MPD' on 7800 Family Manager Set v3.02 
      Installation Disk could not be found ...".  Type a:\win9x in the Copy
      Files from the edit box and click OK.  The driver is now installed.
    
    9 You must restart your computer for the changes to take effect.  Click 
      Yes to restart your computer.  Click No to return to the system 
      properties window.

    (NOTE: If you attempt to re-update the driver again, at step 3 above
    you will need to select No, click Next, and follow the on-screen
    instructions to re-update.)


=-=-=-=-=-=-=
Known Issues
=-=-=-=-=-=-=

    o In some cases, each channel of a MultiChannel adapter must be 
      updated/installed manually with the aic78xx.mpd driver on a 
      freshly installed Windows 95 system. Please follow the
      instructions listed under "Updating the Driver for Windows 95"
      for each channel.

    o Real mode ASPI drivers from EZ-SCSI are not needed, because
      Windows 95 miniport drivers support most SCSI host adapters and
      SCSI devices.  However, you will need to load the ASPI drivers 
      (including MSCDEX.EXE, if you have CD-ROM drive) if any of the 
      following are true: 
      
      o You are running in MS-DOS mode and need to access your CD-ROM 
        drive.
      
      o You are using a scanner or another SCSI device with CONFIG.SYS
        or AUTOEXEC.BAT based drivers, such as HP's SJIIX.SYS.
        
      o You have an older model SCSI-1 CD-ROM driver that Windows 95 does 
        not support.
      
      o You are using a CD-Recorder drive (however, some newer models of
        CD-Recorder drives can use the embedded Windows drivers).
        
    o Some older models of SCSI CD-ROM drives are not compatible with the 
      embedded Windows 95 CD-ROM driver.  You can add support for the 
      CD-ROM drive by doing the following:
      
      1 Make sure your ASPI real mode drivers (including ASPI8DOS.SYS, 
        ASPICD.SYS and MSCDEX.EXE) are loaded and running from your 
        CONFIG.SYS and AUTOEXEC.BAT files.  Consult your EZ-SCSI 
        installation guide for more details.
      
      2 If step 1 did not work, find the file named CDTSD.VXD in the 
        \windows\system\iosubsys directory and rename it to CDTSD.SAV.
        
    o The mapping between MSCDEX.EXE, which runs in real mode, and the
      Windows 95 CD-ROM driver does not match.  You can correct this in
      one of two ways:
      
      1 Comment out the line that loads mscdex.exe in the autoexec.bat 
        file.
      
      2 Change the /L switch on the line that loads mscdex.exe in the
        AUTOEXEC.BAT file so it assigns the CD-ROM drive the next highest 
        logical drive letter after the hard disk drives.

    o Windows 95 does not support sharing of system interrupts (also
      known as IRQs) between two or more I/O subsystem devices (i.e.
      network interface cards or hard disk adapters such as SCSI host
      adapters). When IRQs are shared between I/O devices, lockups can
      occur while booting. If lockups occur, try moving or removing one
      or more PCI cards from one slot to another and bootup your computer
      again.  If problems continue, refer to your system documentation
      and/or your system technical support for information on adding
      your system configuration.

    o When updating/installing the driver for a host adapter, the 
      Family Manager Set v3.02 will not automatically install both 
      Ultra2 and Ultra/Fast drivers.  If you require both drivers, 
      you will have to install them seperately, as per individual host 
      adapter.  For example, after installing the driver for the 
      AHA-2940U2W, there may be a conflict in the Device Manager
      with an existing or newly-installed Adaptec UltraSCSI or earlier 
      host adapter. To resolve this problem, simply update the driver 
      for the conflicting host adapter with the Family Manager Set 
      v3.02 driver from the Device Manager.



=-=-=-=-=-=-=-=-=-=
Diskette Contents
=-=-=-=-=-=-=-=-=-=

The following files are included in this diskette:

    o \WIN9x\AIC78XX.MPD - 7800 series SCSI miniport for Windows 95/98
    o \WIN9x\AIC78U2.MPD - 7800 series Ultra2 SCSI miniport for Windows 95/98
    o \WIN9x\AIC78XX.INF - Install script used by Windows 95/98 setup
    o \WIN9x\README95.TXT - This file
    o \WIN9x\README98.TXT - Readme file for Windows 98
    o \WIN9x\ADPINSTR.VXD - Instrumentation Helper Virtual Device Driver


=-=-=-=-=-=-=-=-=-=
Contacting Adaptec
=-=-=-=-=-=-=-=-=-=

Electronic Support
-------------------------

Technical information, including product literature, answers to commonly asked 
questions, information on software upgrades and other topics is available 
electronically through the following:

   o Adaptec World Wide Web (WWW) site at http://www.adaptec.com. 
   o File Transfer Protocol (FTP) server at ftp.adaptec.com. 
   o To submit your electronic mail message to Adaptec Technical Support
     use the product support information Webmail form at:
     http://www.adaptec.com/support/webmail.html. 
   o Adaptec USA Bulletin Board Service (BBS) at 408-945-7727; supports up 
     to 28,800 bps (bits per second), 8 data bits, 1 stop bit, no parity. 
     No product literature is available on the Adaptec BBS. 
   o Interactive Fax System at 303-684-3400; available 23 hours a day, 7 
     days a week. The fax system is out of service 1 hour each day. 


Technical and Product Support
--------------------------------------------

   o To speak with a product support representative, call 408-934-SCSI
     (7274), M-F, 6:00 a.m. to 5:00 p.m., Pacific Time. After hours, on
     weekends, and on holidays, product support is also available for a 
     fee at 800-416-8066.
   o For electronic technical support and information about many of 
     Adaptec's other electronic support services, or to use the Adaptec
     Interactive Support System call 800-959-SCSI (7274) or 408-945-2550,
     24 hours a day, 7 days a week.  The system prompts you with 
     questions regarding your problem and then provides step-by-step
     troubleshooting instructions.


Sales and Ordering Information
---------------------------------------------

   o For sales information, call 800-442-SCSI (7274), M-F, 6:00 a.m. to
     5:00 p.m., Pacific Time, or 408-945-8600 and ask for Inside Sales, 
     M-F, 8:00 a.m. to 5:00 p.m., Pacific Time.
   o To order Adaptec software and SCSI cables, call 800-442-SCSI (7274),
     M-F, 6:00 a.m. to 5:00 p.m., Pacific Time.
   o To request additional documentation for Adaptec products, call
     800-934-2766 or 510-732-3829, M-F, 6:00 a.m. to 5:00 p.m., Pacific Time.



