Installation of the ES1938/ES1946 AudioDrive for Windows NT 4.0

 1. Turn the PC ON, wait for Windows NT boot up.
 2. Click the Start button on the taskbar.
 3. Choose the Settings item.
 4. Click the Control Panel item. 
 5. In the Control Panel window, double-click the Multimedia icon.  
 6. In the Multimedia Properties dialog box, click the Devices menu 
    option.
 7. Click the Add button. 
 8. In the Add dialog box, choose the first item - Unlisted or Updated 
    Driver - in the list of available drivers.  Click the OK button.
 9. In the Install Driver dialog box, type 'a:' in the text box, insert
    the driver diskette in a floppy disk drive and click the OK button.
10. In the Add Unlisted or Updated Driver dialog box with information 
    about the ESS AudioDrive model (ES11938/ES1946) and the driver 
    version, click the OK button. 
11. Remove the driver diskette.
12. Restart Windows NT for your changes to take effect. You will be 
    prompted with a dialog box, "Restart Now".
13. Installation is complete.


