	
	This utility is for OEMs or Distributors to modify DMI information in 
	the Super Micro BX/GX motherboard BIOS only.


	OEM or System Manufactures can use SMBWORK to add the DMI information
	into the BIOS. 

	You may use sm2lfash.exe utility in the Flash Utility directory to 
	save the BIOS image or get the latest BIOS from our website at 
	http://www.supermicro.com
	

	Run SMBWORK under Windows, choose Load from ROM File. 
	
	Fill the information in the System Manufacture, Product, 
	Serial No, Version No. ...or Chassis.
	After modification double click OK then choose Save to ROM.
	The new saved BIOS will contain the DMI information you just edited.
	Use sm2flash utility to flash the new BIOS into motherboard.
	

	To verify the DMI information, you may use DMI Browser in this CD or
	use Intel LDCM to see the result.
	
	
	Note : This SMBWORK will only apply to Super Micro BX/GX motherboard only.
	       Do not use this on LX/TX BIOS.
	
	
	
	


